{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист2","Обозначения пружин ОПЕЛЯ","Лист3"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист2","index":0,"n_rows":13,"n_cols":3,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[null,"Пружина задняя ОПЕЛЬ ОМЕГА В – усиленная, она же идет на ОПЕЛЬ КАРАВАН – стандартная. Производитель K+F"]
[null,"Номер по каталогу - 774335  "]
[null,"Количество витков = 8"]
[null,"Lo=290 mm"]
[null,"Dt=17 mm – 4 средних витка"]
[null,"Dt=15 mm – 2 предпоследних витка сверху и снизу"]
[null,"Dt=11 mm – 2 последних витка сверху и снизу, поросячии хвосты."]
[]
[null,"Dy=? mm","Это не померил"]
[null,"Po= ? mm","Это не померил"]
[null,"d = ??? mm","Это не померил"]

{"sheet":"Обозначения пружин ОПЕЛЯ","index":1,"n_rows":7,"n_cols":2,"rows_kept":7,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
["KS","  стандартные (не усиленные) пружины на Омегу А (седан)"]
[]
["LG","  стандартные на Омегу Б (седан) до первого рестайлинга 1998-го (или конца 1997-го) года"]
[]
["LP","  стандартные на Омегу Б (седан) с 1998-го по 2003-й год"]

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}