{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":20,"n_cols":11,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Бензонасос KIA Sportage - БОШ 0 580 453 456"]
[]
["SNR-OES","Pressure\nmax/\n[kPA]","Pressure\nmin/\n[kPA]","Flowrate\nmax/[l/h]","Flowrate\nMin/[l/h]","Current\nmax/[A]","Current\nmin/[A]","Voltage\nmax/[V]","Voltage\nmin/[V]","PLV\nmax/\n[kPA]","PLV\nmin/\n[kPA]"]
["0 580 453 435",400,300,110,10,7.5,"",12.5,6.5,450,""]
["0 580 453 439",350,350,115,12,7,"",12,7,500,800]
["0 580 453 443",400,300,110,10,7.5,"",12,6.5,500,850]
["0 580 453 455",300,250,90,28,4.2,"",12,8,450,650]
["0 580 453 456",300,250,75,18,3.6,"",12,8,450,650]
["0 580 453 459",300,250,90,10,4.7,"",12,7.5,450,850]
["0 580 453 469",300,250,80,10,4.5,"",12,8,450,650]
["0 580 453 471",300,"",105,30,5.8,"",12,7.5,500,750]
["0 580 453 480",300,250,90,28,4.2,"",12,8,450,""]
["0 580 453 487",300,250,75,5,3.8,"",12,8,390,540]
["0 580 453 490",300,300,105,20,5,null,12,8,450,750]
["0 580 453 492",300,250,75,5,3.8,"",12,8,390,""]
["0 580 453 494",350,350,115,12,7,"",12,7,500,""]
[]
[]
[]
["Секта насоса Airtex FS154"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}